There are a few limitations:

Dennard scaling – Voltage cannot go too low

Leakage power – Transistor may leak off power even though it doesn’t switch

High temperatures – Temperature may go higher and higher to melt the chips.

Power wall – When the number of density of transistors go up, the power consumption increases, which causes the high temperature issue.

Threshold voltage – voltage scaling is limited because of the noise and threshold voltage